STORE WALK AROUND

**30 DAY MANDATORY CHECKLIST**

STORE\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DATE \_\_\_\_\_\_\_\_ EMPLOYEE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 OK ACTION REQ

Inspect all fire extinguishers on site and trucks for charge \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Inspect and operate all compressor pop off valve \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

 In shop and on service trucks

Summer months treat outdoor tires and yards for bugs. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Inspect all containers for proper labeling on site. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Inspect all grinders, presses, and fans for guards. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Inspect A/C-Heating filters for replacement. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Test eye wash stations for operation. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

General inspection of automotive lifts, ie: fluid leaks \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Frayed cables, missing hardware, oil levels, overall condition

Action required on above items

1. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Completion of above action \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Completion of above action \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**FAX TO 316-522-5166 ATTENTION MIKE HULL, MONTHLY**